This example should be used if you need to explicitly set the buffer size on a continuous acquisition.  An example of why you may need to do this is if you're getting buffer overflow errors when using the default values or if you have specific memory concerns and you want to use a smaller buffer size than automatically configured by DAQmx.

===========================================================================
List of files contained in this ZIP file
===========================================================================
* Cont Acq&Graph Voltage-(explicit buffer).vi --> NOTE: After unzipping, run this program.

===========================================================================
Note: This ZIP file only contains the example code and auxiliary files
      themselves, and does not contain necessary drivers nor standard
      distribution libraries.   Please make sure the standard distribution
      libraries are already on your system before running these examples.
